**Product Codes for Transtemp 03 Feb 22**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sensor Type** | **Product Code** | **ID in Programme** | **Range of temperature** | **Ports** |
| Standards | K101 | C1-FB | -35⁰ C to 40⁰C | P0(4) P1(4) |
| Credit Cards | K114A | C1-AF or 9D | -35⁰ C to 40⁰C | P1(4) |
| Blood Banks | K101B | C1-8D- (0B) | -35⁰C to 40⁰c | P1(7) P2 (6) |
| Digitals | K101A REV.C | CB | -35⁰C to 40⁰c | P1(4) |
| Humidity’s | FK102 | C6 | 0 ⁰C to 50⁰C | P0(3) |
| Humidity’s | FK102 | C6 | 30% to 80% | P1(3) |
| Oxygen Sensor | K105-02 | E5 |  |  |
| C02 | K105-C02 | E6 |  |  |
| Battery Cyro | K105T | CA | -200⁰C to +200⁰C | P2(12) |
| AMP Cyro | K105TAmp | C7 | -210⁰C to 30⁰C | P2 (14) |
| Door Ajar | K101DA | CC | -35⁰ C to 40⁰C | P0(4) P1(4) |
| Hot Sensor | K101B | C1-8D (CD) | -10⁰ C to 100⁰C | P2(10) |
| Cold Thermist | K101PEC | C1-FB (CC) | -35⁰ C to 40⁰C | P1 |